| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
ADC Attributes
VK DAQ Attribute » VE3664L

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
Resolution | Read |  | 24 | bit | AIN resolution
SamplingFrequency | Read|Write | 0.001~102400.000 | 100000 | SPS | AIN sampling frequency
SamplingSize | Read|Write | 0~4294967295 | 4294967295 |  | 4294967295: Continuous Acquisition 0~4294967294: Finite Acquisition
SamplingStatus | Read | 0,1 | 0 |  | 0: Not collecting anymore 1:Collecting
TransferMode | Read|Write | Online,Offline | Online |  | Transfer mode
TriggerMode | Read|Write | Default,Posedge,Negedge, HighLevel,LowLevel | Default |  | Trigger mode Default: No trigger Posedge: Rising edge trigger Negedge: Falling edge trigger HighLevel: High level trigger LowLevel: Low level trigger
TriggerSource | Read|Write | DIN1.1 | DIN1.1,DIN1.1,AIN1,AIN2,AIN3,AIN4 |  | Trigger source