| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Frequency Attributes
VK DAQ Attribute » VE3664L

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Frequency2 for counting
  Must be set:Dio1.2Mode = DigitalInput<br>

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
FrequencyList | Read | Frequency2 |  |  | List of available Frequency devices
Frequency2 | Read|Write | 1.000~100000.000 | 0 |  | Read: Returns the count value of rotary Frequency 2 connected to Dio1.2 Write: Write any value to clear the count value of rotary Frequency 2 connected to Dio1.2