| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Counter Attributes
VK DAQ Attribute » VE3664_VE3662

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Counter1 for counting
  Must be set:Dio1.1Mode = DigitalInput<br>

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
Counter1 | Read|Write | 0~Counter1Max | 0 |  | Read: Returns the Dio1.1 input pulse count value Write: Write any value to clear the Dio1.1 input pulse count value
Counter1Max | Read|Write | 0~4294967295 | 4294967295 |  | Counter1 maximum value