| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Frequency Attributes
VK DAQ Attribute » VK7016_VK7018

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Frequency1
  Must be set:Dio1.1Mode = DigitalInput

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
FrequencyList | Read | Frequency1,Frequency2, Frequency3,Frequency4 |  |  | List of available Frequency for the device
Frequency1 | Read|Write |  | 0 |  | Read: Return Dio1.1 frequency value Write: Write any value to clear Dio1.1 frequency value
Frequency2 | Read|Write |  | 0 |  | Read: Return Dio1.2 frequency value Write: Write any value to clear Dio1.2 frequency value
Frequency3 | Read|Write |  | 0 |  | Read: Return Dio1.3 frequency value Write: Write any value to clear Dio1.3 frequency value
Frequency4 | Read|Write |  | 0 |  | Read: Return Dio1.4 frequency value Write: Write any value to clear Dio1.4 frequency value