| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
VE3662 Channel Attributes

Note
  VE3662 Channel list:
  AIN1:2
  MIN1
  DIN1

Name | Applicable channels | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | --- | ---
AccelSensitivity | AIN1:2 | Read|Write |  | 0.05 |  | Acceleration sensor sensitivity
Bandwidth | AIN1:2 | Read |  | 20400 | Hz | Bandwidth
InputRange | AIN1:2 | Read|Write | 0~10.0000000000 | 10.0000000000 | V | Input range
InputType | AIN1:2 | Read|Write | Differential,SingleEnded, IEPE,Current | SingleEnded |  | Differential: Differential voltage input SingleEnded: SingleEnded voltage input IEPE: IEPE input Current: Current input Tip: Due to hardware differences at the input end, the supported input types are. Please read the channel property: InputTypeAvailable
Raw | AIN1:2 MIN1 DIN1 | Read Read Read |  |  |  | AIN1:4 raw value MIN1 raw value DIN1 raw value
Rsense | AIN1:2 | Read |  | 250 | Ω | The resistance of the sampling resistor is only applicable to current input type
Save | AIN1:2 MIN1 DIN1 | Read|Write Read|Write Read|Write Read|Write |  | Disable |  | AIN1:2 offline saving MIN1 offline saving DIN1 offline saving
ScaleDivisor | AIN1:2 | Read Read |  | 1000000.000000 |  | AIN1:2 Scale divisor
ScaleMultiplier | AIN1:2 | Read Read |  | 1.38716264 |  | AIN1:2 Scale multiplier
Voltage | AIN1:2 | Read Read|Write |  |  | V | Voltage
Source | MIN1 | Read|Write | VirtualCounter | VirtualCounter |  | MIN1 Data source selection VirtualCounter: Virtual counter value