| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Pwm Attributes
VK DAQ Attribute » VP6088

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Pwm1
  Must be set:Dio1.1Mode = Pwm
  Set PWM duty cycle: Pwm1DutyCycle = 0.5
  Set PWM carrier frequency: Pwm1CarrierFrequency = 10

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
Pwm1CarrierFrequency | Read|Write | 0.050~1000000.000 | 1 |  | Pwm1 carrier frequency output from Dio1.1
Pwm1DutyCycle | Read|Write | 0.000000000000~1.000000 | 0 |  | Pwm1 duty cycle output from Dio1.1
Pwm2CarrierFrequency | Read|Write | 0.050~1000000.000 | 1 |  | Pwm2 carrier frequency output from Dio1.2
Pwm2DutyCycle | Read|Write | 0.000000000000~1.000000 | 0 |  | Pwm2 duty cycle output from Dio1.2
Pwm3CarrierFrequency | Read|Write | 0.050~1000000.000 | 1 |  | Pwm3 carrier frequency output from Dio1.3
Pwm3DutyCycle | Read|Write | 0.000000000000~1.000000 | 0 |  | Pwm3 duty cycle output from Dio1.3
Pwm4CarrierFrequency | Read|Write | 0.050~1000000.000 | 1 |  | Pwm4 carrier frequency output from Dio1.4
Pwm4DutyCycle | Read|Write | 0.000000000000~1.000000 | 0 |  | Pwm4 duty cycle output from Dio1.4