| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
ADC Attributes
VK DAQ Attribute » VP6088

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
PretriggerSampleSize | Read|Write | 0~762600 | 0 |  | Number of sampling points before triggering sampling
Resolution | Read |  | 24 | bit | AIN resolution
SamplingFrequency | Read|Write | 0.001~204800.000 | 100000 | SPS | AIN sampling frequency
SamplingSize | Read|Write | 0~4294967295 | 4294967295 |  | 4294967295: Continuous Acquisition 0~4294967294: Finite Acquisition
SamplingStatus | Read | 0,1 | 0 |  | 0: Not collecting anymore 1:Collecting
TransferMode | Read|Write | Online,Offline | Online |  | Transfer mode
TriggerMode | Read|Write | Default,Posedge,Negedge, HighLevel,LowLevel,MultiEdge | Default |  | Trigger mode Default: No trigger Posedge: Rising edge trigger Negedge: Falling edge trigger HighLevel: High level trigger LowLevel: Low level trigger MultiEdge: Multilateral edge triggering
TriggerSource | Read|Write | DIN1.1,DIN1.2,DIN1.3,DIN1.4, MIN1,MIN2, AIN1,AIN2,AIN3,AIN4 | DIN1.1 |  | Trigger source
VirtualCounter | Read|Write | 0~VirtualCounterMax | 0 |  | Read: Returns the virtual counter value Write: Writes any value to clear the virtual counter value
VirtualCounterMax | Read|Write | 0~4294967295 | 4294967295 |  | Virtual counter maximum value
VirtualTimerInterval | Read|Write | 0~4294967295 |  | sec | Virtual timer interval
VirtualTimerValue | Read|Write |  | 0 | sec | Virtual timer value