| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Temp Attributes
VK DAQ Attribute » VP8388_VP8384

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Temp1
  Must be set:Dio1.1Mode = Ds18b20

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
TempList | Read | Temp1,Temp2,Temp3,Temp4 |  |  | List of available Temp for the device
Temp1 | Read |  |  | 0.001°C | Read examples: w1_bus_master1_28_3ce1e3803dd1_32523 w1_bus_master1: Dio1.1 1-Wire bus 28: Family code 3ce1e3803dd1: Serial number 32523: 32.523°C
Temp2 | Read |  |  | 0.001°C | Read examples: w1_bus_master2_28_3ce1e3803dd1_32523 w1_bus_master2: Dio1.2 1-Wire bus 28: Family code 3ce1e3803dd1: Serial number 32523: 32.523°C
Temp3 | Read |  |  | 0.001°C | Read examples: w1_bus_master3_28_3ce1e3803dd1_32523 w1_bus_master3: Dio1.3 1-Wire bus 28: Family code 3ce1e3803dd1: Serial number 32523: 32.523°C
Temp4 | Read |  |  | 0.001°C | Read examples: w1_bus_master4_28_3ce1e3803dd1_32523 w1_bus_master4: Dio1.4 1-Wire bus 28: Family code 3ce1e3803dd1: Serial number 32523: 32.523°C