| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
System Attributes
VK DAQ Attribute » VE3664L

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
DeviceMode | Read|Write | Slave,Master | Master |  | Slave: Collect an AIN data point when receiving the rising edge of the Sync pulse Master: Outputs a pulse from Sync for each AIN data point acquired For multi-card synchronous acquisition: One card is set as Master to output synchronization pulses, and the other cards are set as Slave to receive synchronization pulses For external clock acquisition: Set as Slave
DeviceStatus | Read | Unavailable,Available | Available |  | Check if the device is available
Eth0Status | Read | Determined by the actual connection situation |  |  | Read examples: negotiated 1000baseT-FD flow-control, link ok negotiated: determine the connection parameters through automatic negotiation 1000baseT-FD: Gigabit Ethernet full-duplex mode flow-control: enable flow control link ok: the network connection is normal
Hostname | Read|Write |  | DAQ-VE3664L-081125 |  | Hostname
InternalTemp | Read |  |  |  | Read the internal temperature in Celsius ℃
MachineId | Read |  |  |  | A string of 32 HEX characters. Each acquisition card has a unique machine ID.
Model | Read | vp3668 |  |  | Model
Network | Read|Write | Determined by the actual connection situation |  |  | Read examples: dhcp,ip=192.168.1.199,gateway=192.168.1.1,netmask=255.255.255.0,mac=c8:d8:f9:00:03:63 static,ip=192.168.1.199,gateway=192.168.1.1,netmask=255.255.255.0,mac=c8:d8:f9:00:03:63 Write examples: dhcp dhcp,mac=c8:d8:f9:00:03:63 static,ip=192.168.1.222,gateway=192.168.1.1,netmask=255.255.0.0 static,ip=192.168.1.222,gateway=192.168.1.1,netmask=255.255.0.0,mac=c8:d8:f9:00:03:63
SystemTime | Read|Write | YYYY-MM-DD hh:mm:ss |  |  | System time
UsbOtgStatus | Read | Host,Device |  |  | Usb Otg Status
Version | Read |  |  |  | AIN firmware version
Vref | Read |  | 4.000 | V | AIN reference voltage