| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DAC Attributes
VK DAQ Attribute » VP6088

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
AoutConstantStop | Read|Write | Null,StopWait,StopNow,StopZero | Null |  | Stopping method in Aout continuous output mode: Null:In discontinuous output mode StopWait:After outputting the last set of waveforms StopNow:Immediately stop outputting voltage at that time StopZero:Immediately stop and output 0V voltage
AoutMode | Read|Write | Normal,Constant | Normal |  | Aout output mode: Normal:Repeatedly outputting fixed waveform patterns Constant:Continuously output any waveform mode
AoutReset | Read|Write | permit | permit |  | Write 'permission' to reset the DAC
AoutResolution | Read | 16 | 16 |  | DAC effective bit
AoutSamplingFrequency | Read|Write | 0.1~128000.0 | 128000 |  | The point frequency output by DAC, for example: In the continuous output of any waveform mode, the DAC needs to output 51200 points of data every second. Set this input to 51200 to achieve this
AoutVersion | Read |  |  |  | Aout firmware version
AoutVref | Read |  | 4.096 | V | Aout reference voltage