| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-TriggerOutput Attributes
VK DAQ Attribute » VP8388_VP8384

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Set Dio1.1 to trigger output pulse mode
  Must be set:Dio1.1Mode = TriggerOutput

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
TriggerOutputLevel | Read|Write | LowLevel,HighLevel | LowLevel |  | Indicates the trigger output pulse level: LowLevel: triggers the output pulse to be low level HighLevel: triggers the output pulse to be high level
TriggerOutputWidth | Read|Write | 0.000000~1.000000 | 0.01000 | s | Trigger output pulse width