| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Counter Attributes
VK DAQ Attribute » VE3668

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Counter1 for counting
  Must be set:Dio1.1Mode = DigitalInput<br>

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
CounterList | Read | Counter1,Counter2 |  |  | List of available Counter devices
Counter1 | Read|Write | 0~65536 | 0 |  | Read: Returns the count value of rotary Counter 1 connected to Dio1.1 Write: Write any value to clear the count value of rotary Counter 1 connected to Dio1.1
Counter2 | Read|Write | 0~65536 | 0 |  | Read: Returns the count value of rotary Counter 2 connected to Dio1.2 Write: Write any value to clear the count value of rotary Counter 2 connected to Dio1.2