| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Basic Attributes
VK DAQ Attribute » VE3664L

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:using Dio1.1 for level acquisition
  Must be set:Dio1.1Mode = DigitalInput<br>
  For example:using Dio1.1 for level output
  Must be set:Dio1.1Mode = DigitalOutput

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
DioList | Read | Dio1.1,Dio1.2,Dio1.3,Dio1.4 |  |  | List of available DIO devices
Dio1Data | Read|Write | 0~15 | 15 |  | Dio data value bit0: Dio1.1 data value bit1: Dio1.2 data value bit2: Dio1.3 data value bit3: Dio1.4 data value
Dio1.1Data | Read|Write | 0,1 | 1 |  | Dio1.1 data value 0: Low level 1: High level
Dio1.1Mode | Read|Write | DigitalInput,DigitalOutput,Pwm | DigitalInput |  | Dio1.1 mode DigitalInput: Dio1.1 used for level input, pulse counting, etc DigitalOutput: Dio1.1 used for level output Pwm: Dio1.1 used for pulse width modulation output
Dio1.2Data | Read|Write | 0,1 | 1 |  | Dio1.2 data value 0: Low level 1: High level
Dio1.2Mode | Read|Write | DigitalInput,DigitalOutput,Pwm | DigitalInput |  | Dio1.2 mode DigitalInput: Dio1.2 used for level input, pulse counting, etc DigitalOutput: Dio1.2 used for level output Pwm: Dio1.2 used for pulse width modulation output
Dio1.3Data | Read|Write | 0,1 | 1 |  | Dio1.3 data value 0: Low level 1: High level
Dio1.3Mode | Read|Write | DigitalInput,DigitalOutput | DigitalInput |  | Dio1.3 mode DigitalInput: Dio1.3 used for level input DigitalOutput: Dio1.3 used for level output
Dio1.4Data | Read|Write | 0,1 | 1 |  | Dio1.4 data value 0: Low level 1: High level
Dio1.4Mode | Read|Write | DigitalInput,DigitalOutput | DigitalInput |  | Dio1.4 mode DigitalInput: Dio1.4 used for level input DigitalOutput: Dio1.4 used for level output