| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
DIO-Encoder Attributes
VK DAQ Attribute » VP6088

Note
  Need to modify the corresponding Dio1.xMode to the required type
  For example:Use Encoder1 for counting
  Must be set:Dio1.1Mode = DigitalInput
  Must be set:Dio1.2Mode = DigitalInput<br>
  For example:Use Encoder2 for counting
  Must be set:Dio1.3Mode = DigitalInput
  Must be set:Dio1.4Mode = DigitalInput<br>

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
Encoder1 | Read|Write | 0~Encoder1Max | 0 |  | Read: Returns the count value of rotary encoder 1 connected to Dio1.1 and Dio1.2 Write: Write any value to clear the count value of rotary encoder 1 connected to Dio1.1 and Dio1.2
Encoder1Max | Read|Write | 0~4294967295 | 4294967295 |  | Encoder1 maximum value
Encoder2 | Read|Write | 0~Encoder2Max | 0 |  | Read: Returns the count value of rotary encoder 2 connected to Dio1.3 and Dio1.4 Write: Write any value to clear the count value of rotary encoder 2 connected to Dio1.3 and Dio1.4
Encoder2Max | Read|Write | 0~4294967295 | 4294967295 |  | Encoder2 maximum value