| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
VK7016 Channel Attributes
VK DAQ Attribute

Note
  VK7016 Channel list:
  AIN1:16
  MIN1:2
  DIN1
  AOUT1:2

Name | Applicable channels | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | --- | ---
AccelSensitivity | AIN1:16 | Read|Write |  | 0.05 |  | Acceleration sensor sensitivity
Bandwidth | AIN1:16 | Read |  | 43300 | Hz | Bandwidth
FilterType | AIN1:16 | Read|Write | Wideband,Sinc | Sinc |  | Wideband: Wideband digital filter Sinc: Sinc digital filter
InputRange | AIN1:16 | Read|Write | 0~10.00000000 | 10.00000000 | V | Input range
InputType | AIN1:16 | Read|Write | Differential,SingleEnded, IEPE,Current | Differential |  | Differential: Differential voltage input SingleEnded: SingleEnded voltage input IEPE: IEPE input Current: Current input Tip: Due to hardware differences at the input end, the supported input types are. Please read the channel property: InputTypeAvailable
Raw | AIN1:16 MIN1:2 DIN1 AOUT1:2 | Read Read Read Read |  |  |  | AIN1:16 raw value MIN1:2 raw value DIN1 raw value AOUT1:2 raw value
Rsense | AIN1:16 | Read |  | 250 | Ω | The resistance of the sampling resistor is only applicable to current input type
SamplingSize | AOUT1:2 | Read|Write | 0~4294967295 | 4294967295 |  | 4294967295: Continuous Acquisition 0~4294967294: Finite Acquisition
ScaleDivisor | AIN1:16 AOUT1:2 | Read Read |  | 1.953125000 305.17578125 |  | AIN1:16 Scale divisor AOUT1:2 Scale divisor
ScaleMultiplier | AIN1:16 AOUT1:2 | Read Read |  | 1000000 1000000 |  | AIN1:16 Scale multiplier AOUT1:2 Scale multiplier
TriggerLevel | AIN1:16 MIN1:2 | Read|Write | AIN:-10.00000000~10.00000000 MIN:0~4294967295 | AIN:0.00000000 MIN:0 | V | AIN1:16 Analog trigger voltage value MIN1:2 Trigger value
VirtualCounter | AOUT1:2 | Read|Write | 0~4294967295 | 0 |  | Read: Returns the virtual counter value Write: Writes any value to clear the virtual counter value
VirtualTimerInterval | AOUT1:2 | Read|Write | 0~4294967295 |  | sec | Virtual timer interval
VirtualTimerValue | AOUT1:2 | Read|Write |  | 0 | sec | Virtual timer value
Voltage | AIN1:16 AOUT1:2 | Read Read |  |  | V V | Voltage Voltage
Waveout | AOUT1:2 | Read|Write | Disable,Enable | Enable |  | Disable: AOUT1:2 Disable wave out Enable: AOUT1:2 Enable wave out
Source | MIN1:2 | Read|Write | VirtualCounter, Counter1,Counter2,Counter3,Counter4, Encoder1,Encoder2 | VirtualCounter |  | MIN1:2 Data source selection VirtualCounter: Virtual counter value Counter1: Dio1.1 input pulse count value Counter2: Dio1.2 input pulse count value Counter3: Dio1.3 input pulse count value Counter4: Dio1.4 input pulse count value Encoder1: Count value of rotary encoder 1 connected to Dio1.1 and Dio1.2 Encoder2: Count value of rotary encoder 2 connected to Dio1.3 and Dio1.4