| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
Functions
Get task
libvkdaq Function interface » Configuration task

## Functions
int32_t | VkDaqGetTasks (char tasks[], int32_t size)
| Get task.

## Detailed Description

## Function Documentation

## ◆ VkDaqGetTasks()

int32_t VkDaqGetTasks | ( | char | tasks[],
|  | int32_t | size
| ) |  |

Get task.

data type | parameter | describe
--- | --- | ---
`char[]` | `tasks[]` | A character array used to store task names, separated by commas between multiple values.
`int32` | `size` | The size of the task array.

Returns
  On success, return value >= 0.
  On failure, returns a negative error number.For detail, please Call VkDaqGetLastErrorInfo

C language reference
#include <stdio.h>
#include "libvkdaq.h"
int main(int argc, char* argv[])
{
char tasks[256] = { 0 };
int32_t size = sizeof(tasks);
int32_t result = VkDaqGetTasks(tasks, size);
printf("tasks= %s ,size= %d \n", tasks,size);
if (result >=0 ) {
printf("Successful\n");
}
else {
printf("Failed\n");
}
return 0;
}
VkDaqGetTasks
int32_t VkDaqGetTasks(char tasks[], int32_t size)
Get task.