| libvkdaq VKINGING DAQ Library API Reference |

Loading...
Searching...
No Matches
Offline Attributes
VK DAQ Attribute » VK7016_VK7018

Name | Read|Write | Available Value | Factory Value | Unit | Remark
--- | --- | --- | --- | --- | ---
OfflineMode | Read | Null,ContAcq,TriggerContAcq,TriggerAcq, TimerAcq,LevelAcq | Null |  | Offline storage mode
OfflineStatus | Read | Disable,Enable | Disable |  | Offline Status
OfflineSaveDirectory | Read |  |  |  | SD card directory, for example: mmcblk0p1/media/root/76AF-5085
SaveFormat | Read|Write | bin,csv | bin |  | Offline saved data format0: bin: binary csv: text
SaveTime | Read|Write | 5~3600 | 5 |  | The time of offline saving for each file
TfCardStatus | Read | Removed,Inserted,Ready |  |  | Tf Card Status